**Smart Deploy 🡪** imaging server

Win7

Win10

Make sure that Network boot is enabled in the BIOS

Smart Deploy IP 🡪 192.168.1.22

Network Boot for HPCE 8300 🡪 f12

BIOS setup 🡪 f10

**Setup** 🡪 Security 🡪 Network Boot or PXE Boot = Enable 🡪Save 🡪Restart (ctrl alt del)

**Steps**

Deploy and Image🡪Recreate Drives

**Computer name**: fse-modelNum-sequentialNum

**Example**: fse-HPE8300-5

Fse-data -hp-model track

Check Computer Name

* Five Star
* FSE Clients
* Type the Computer Name

**Domain** – tutorperini.com

**Organization Unit** – FSEPClients.OU=\...

Username: tutorperini\richard.hahn

Password: Welcome123